
*****************************************************************************
*                                                                           *
*           Microsoft Windows 2000 Installation                             *
*             for PCMCIA Fast Ethernet Card                                 *
*                                                                           *
*****************************************************************************


       Windows 2000 provides a complete "Plug and Play" System that will
       automatically recognize and configure most PC Cards.

       Before inserting your PCMCIA Fast Ethernet PC Card, please have the
       installation media for the Windows 2000 ready for any request for files.

Windows 2000 Setup

(1)  With the system off, remove all PC Cards.

(2)  Start up your computer.  After Windows 2000 is up and running,
     put the driver disk of PCMCIA Fast Ethernet into drive A:.

(3)  Insert PCMCIA Fast Ethernet Card into PC Card slot.

(4)  When the Found New Hardware Wizard window appears, click on the
     "Next" button.

(5)  Select "Floppy disk drive" item and click the "Next" button.
     Windows 2000 will check the disk that is in the floppy drive
     for the PCMCIA Fast Ethernet Card network drivers.

(6)  When the Fast Ethernet PC Card message appears on the "Driver File Search
     Results" screen, click the "Next" button.
     Windows 2000 will begin copying files.

(7)  You may get a warning message said "Microsoft has not digitally signed
     the software you wanted to install. Do you want to continue the
     installation?". Click "Yes" to continue the installation.

(8)  Click the "Finish" button.

(9) Restart the computer.

