
*****************************************************************************
*                                                                           *
*           Microsoft Windows for Workgroup 3.11 Installation               *
*           for PCMCIA Fast Ethernet Adapter                                *
*                                                                           *
*****************************************************************************

Installation Procedures:

  NDIS3 Driver for Workgroup
        1. Click on "Network Setup" icon in "Network" program group.
        2. In "Network Settings" dialog box, click mouse on
           "Networks..." button to select the network operating
           system.
        3. In "Networks" dialog box, check the radio button before
           "Install Microsoft Windows Network" and "No Additional
           Network". Press OK to go back the Network Settings screen.
        4. Click on "Drivers..." button to select network driver.
        5. In "Network Drivers" dialog box, press "Add Adapter..."
           button to enter "Add Network Adapter" dialog box. Select
           "Unlisted or Updated Network Adapter" and press OK.
        6. Windows will prompt a "Install Driver" dialog box. In this
           time, put the software diskette into floppy drive and
           press OK.
        7. Select the "Enhanced mode NDIS3 for...." string and press OK.
        8. Follow Windows instructions to complete the installation
           and exit Windows.
        9. Run INSTALL.EXE from driver diskette's root directory.
       10. Select "Windows for Workgroup" in "Network Operating System"
           screen and enter "Driver Install" screen.
       11. If current settings are acceptable, select "Start
           Installation" and go to step 13.  Otherwise, select
           "Modify Parameters" to make settings changed.
       12. Move cursor to focus on the setting you want to make
           change and press Enter to select a fit value. When the
           configuration is accepted, press Enter on the OK field to
           exit the screen.  Back to step 11.
       13. Select "NDIS Server(LAN Manager,...)" as the network
           server you will attach to and press Enter key.
       14. Installation program starts copying related files from
           diskette to the destination directory and modifies
           AUTOEXEC.BAT and NET.CFG under user's agreement.
       15. Installation is complete.  Please reboot the computer to
           have the driver take effect.


  NDIS2 Driver for Workgroup
        1. Click on "Network Setup" icon in "Network" program group.
        2. In "Network Settings" dialog box, click mouse on "Networks..."
           button to select the network operating system.
        3. In Networks dialog box, check the radio button before
           "Install Microsoft Windows Network" and "No Additional
           Network".  Press OK to go back the Network Settings screen.
        4. Click on "Drivers..." button to select network driver.
        5. In "Network Drivers" dialog box, press "Add Adapter..." button
           to enter "Add Network Adapter" dialog box. Select "Unlisted or
           Updated Network Adapter" and press OK.
        6. Windows will prompt a "Install Driver" dialog box.  In this
           time, put the software diskette into floppy drive and press OK.
        7. Select the "Real mode NDIS2 for...." string and press OK.
        8. Follow Windows instructions to complete the installation and
           exit Windows.
        9. Run INSTALL.EXE from driver diskette's root directory.
       10. Select "Windows for Workgroup" in "Network Operating System"
           screen and enter "Driver Install" screen.
       11. If current settings are acceptable, select "Start
           Installation" and go to step 13. Otherwise, select "Modify
           Parameters" to make settings changed.
       12. Move cursor to focus on the setting you want to make
           change and press Enter to select a fit value.  When the
           configuration is accepted, press Enter on the OK field to
           exit the screen.  Back to step 11.
       13. Select "NDIS Server(LAN Manager,...)" as the network server
           you will attach to and press Enter key.
       14. Installation program starts copying related files from
           diskette to the destination directory and modifies
           AUTOEXEC.BAT and NET.CFG under user's agreement.
       15. Installation is complete.  Please reboot the computer to
           have the driver take effect.


  ODI Driver for Workgroup
        1. Click on "Network Setup" icon in "Network" program group to install
           network driver.
        2. In Network Settings dialog box, click mouse on
           "Networks..." button to select the network operating system.
        3. In "Networks" dialog box, check the radio button before
           "Install Microsoft Windows Network" and "Others:".
           Then select one of Netware Shell, 3.X or 4.0 and above,
           and press OK to go back the "Network Settings" screen.
        4. Click on "Drivers..." button to select network driver.
        5. In Network Drivers dialog box, press "Add Adapter..."
           button to enter "Add Network Adapter" dialogbox. Select
           "Unlisted or Updated Network Adapter" and press OK.
        6. Windows will prompt a "Install Driver" dialog box. In this
           time, put the software diskette into floppy drive and press OK.
        7. Select the "Netware ODI Driver ...." string and press OK.
        8. Follow Windows instructions to complete the installation
           and exit Windows.
        9. Run INSTALL.EXE from driver diskette's root directory.
       10. Select "Windows for Workgroup" in "Network Operating System"
           screen and enter "Driver Install" screen.
       11. If current settings are acceptable, select "Start
           Installation" and go to step 13.  Otherwise, select
           "Modify Parameters" to make settings changed.
       12. Move cursor to focus on the setting you want to make change
           and press Enter to select a fit value.
           When the configuration is accepted, press Enter on the OK
           field to exit the screen.  Back to step 11.
       13. Select "Novell Netware Server" as the network server you
           will attach to and press Enter key.
       14. Installation program starts copying related files from
           diskette to the destination directory and modifies
           AUTOEXEC.BAT and NET.CFG under user's agreement.
       15. Installation is complete.  Please reboot the computer to
           have the driver take effect.

