
*****************************************************************************
*                                                                           *
*           Microsoft Windows NT Installation                               *
*             for PCMCIA Fast Ethernet Card                                 *
*                                                                           *
*****************************************************************************

  This document contains the installation guide for the Microsoft
  Windows NT Operating System.

  It is recommented to print the instruction out on a printer before
  installation.  For the best results, open this document in Windows
  Write, Microsoft Word, or another word processing application, select
  the entire document and format the text in 10 point Courier before
  printing.


  Windows NT Version 4.0
  =======================================

  1.  Open the Control Panel, and choose Network Setup.

  2.  When the Network window appears, click on the
       Adapters tab.  Click on the Add button, followed by
       Have Disk.  Put the driver disk into drive A.
       When asked to supply the path to the disk, type a:\
       and click OK.

       NT will ask you to supply the I/O Base,
       Interrupt, and Memory values for the card.
       Good values to start with are 300 (for the
       I/O Base) and 5 (for the IRQ).

  3.  When you're finished, click OK.  NT will copy
       necessary files to your computer.

  4.  When the Network window reappears, click on the
       Bindings tab.  Choose your bindings.  Click on the
       Protocols tab and select your settings.  Do the same
       for the Services tab.

  5.  After your bindings, settings, and services are set,
       click on the Close button.  Choose to restart your
       computer.  After NT restarts, be sure to log in.



  Windows NT Version 3.51
  =======================================

  1.  Open the Control Panel, and choose Network Setup.

  2.  Click the Add Adapter button.

  3.  Select "<Other> Requires disk from manufacturer".

  4.  Insert Driver Diskette in Drive A: and type A:\ in the path.

  5.  Select "PCMCIA Fast Ethernet Adapter" from the list.

  6.  Set the IRQ level, I/O Port and Memory Base Address to the desired
      settings from the lists of free resources available. And click OK.

  8.  Click OK to exit Network Setup.

  9.  Insert the PCMCIA Fast Ethernet Card and Reboot Windows NT.

