| Dual Serial I/O Setup Center
| Welcome
| Main
| •Install
| •Documents
| •3rd Party Apps
Windows CE |
README
INSTALL
Click Install to launch the I/O setup program for a Windows CE device. When software installation is complete, disconnect the mobile computer from the host PC. Soft reset the mobile computer by pressing the reset button. If you would like additional information about this software, click the Readme button or see the User's Guide.
Windows 95OB/98/Me/2000/XP |
README
To install the Hi-Speed Serial software, insert the Dual I/O HS Serial Card into your computer and wait for the "Found New Hardware Wizard". Follow the Wizard instructions using the default (Recommended) options to complete the installation. Depending on your computer's operating system, you may need to complete the Wizard 2 or 3 times. Complete the Wizard again each time it launches until all the necessary files are installed. For step-by-step installation instructions, please see the User's Guide.
| © Copyright 2001-2003, Socket Communications, Inc. All rights reserved.