
                 PCMCIA Fast Ethernet Card Installation
                        for Personal Netware

 Contents
 --------
        .Introduction
        .Requirements
        .Minimum Skill Level
        .Getting Started

 Introduction
 ------------
        The ODI driver program allows you to run multiple protocol stacks
        and install up to two network adapters in a workstation. This ODI
        driver supports the Port, Node Address, Protocol and Frame options
        for creating your own NET.CFG file. For more information on these
        keywords, please refer to Novell's "NetWare ODI shell for DOS -
        NET.CFG options". This installation assumes that the PCMCIA drivers
        are working properly.

 Requirements
 ------------
        .A PCMCIA compatible Laptop
        .A PCMCIA chipset that is PCIC compatible (Intel, Cirrus, Vadem, and
         VLSI) or a Card Service has been installed
        .Personal Netware network operating system
        .A PCMCIA Fast Ethernet Card
        .A knowledge of basic DOS commands and editing text files

 Minimum Skill Level
 -------------------
        .A knowledge of basic DOS commands
        .A knowledge of editing text files
        .A knowledge of DOS basic file structure (CONFIG.SYS and AUTOEXEC.BAT)
        .A knowledge of the network driver configuration being used
        .Please see Support Options if you are not comfortable will this
         skill level

 Getting Started
 ---------------
        1. Follow the normal installation procedure as described by Personal
           Netware.
        2. It will prompt the user for a network driver choose "Other Network
           support driver".
        3. It will request a path for the drivers. Respond with the path of
           the ODI DOS driver, .INS file, and NET.CFG sample installed with
           this readme.
        4. Run STARTNET to access the Novell network.

