
    Artisoft Lantastic 6.0 Installation

            1. Install LANTASTIC 6.0 first.
            2. Run INSTALL.EXE from driver diskette's root directory.
            3. Select "LANTASTIC 6.0" in "Network Operating System" screen
               and enter "Driver Install" screen.
            4. If current settings are acceptable, select "Start
               Installation" and go to step 6. Otherwise, select "Modify
               Parameters" to make settings changed.
            5. Move cursor to focus on each field you want to make change
               and press Enter to select a fit value.  Then press Enter
               on the OK field to go back the step 4.
            6. Installation program starts copying related files from
               diskette to the destination directory and modifies
               CONFIG.SYS, PROTOCOL.INI, and STARTNET.BAT under user's
               agreement.
            7. Installation is complete.  Please reboot the computer to
               have the driver take effect.


