
How to install the NDIS 2.x driver for IBM LAN OS/2 Warp Version 3.


(1)Enable PCMCIA Services under OS/2 Warp Version 3

   Before the NDIS driver being installed, please follow the following
   steps to make sure the PCMCIA Services has been enabled.

    1.In the OS/2 Desktop group, double-click on the <OS/2 System> icon.
    2.double-click on the <System Setup> icon.
    3.double-click on the <Selective Install> icon.
      If the PCMCIA Services was enabled already, you can see the PC
      vendor and model name listed under the <PCMCIA Support> Icon.
      Otherwise, you can see an "No Support Installed" string listed under
      the <PCMCIA Support> Icon. For not enabled case, please follow the
      steps list below to install the PCMCIA Services.
    4.Select the <PCMCIA Support> button.
    5.Select PCMCIA system.
      If the PC model is not on the list, you may select a PC that use
      the same PCMCIA controller with your PC.
      For example :
           Select IBM ThinkPad 750 for Intel 82365 compatible chips.
      If the selected model is incorrect, the PCMCIA function will work
      improperly. You have to unstall the services and to re-install the
      correct one.
    6.Click <OK>.
    7.Click <Install>.
    8.Select the source drive and directory
      For Example D:\OS2IMAGE
    9.Click <Install>.
   10.Click <OK>.


(2)Install NDIS2 driver for IBM LAN Server 4.0

 1.In the OS/2 Desktop group, double-click on the <MPTS> icon.
 2.Click on the <Configure> button.
 3.Select the <LAN adapters and protocols> option.
 4.Click on the <Configure> button.
 5.Select the "Other adapters ..." option.
 6.Insert the driver diskette and type the driver path:
    A:\OS2\NDIS2
   Click on the <OK> button.
 7.Select <PCMCIA Fast Ethernet Adapter>, and then click on the <Add> button.
 8.Select <IBM OS/2 NETBIOS>, and then click on the <Add> button.
 9.Click <OK>.
10.Click <Close>.
11.Click <Exit>.
12.Shutdown and Restart your system.
