
                 PCMCIA Fast Ethernet Card Installation
                       for NetWare Lite Driver

 Contents
 --------
        .Introduction
        .Requirements
        .Minimum Skill Level
        .Getting Started

 Introduction
 ------------
        The ODI driver program allows you to run multiple protocol stacks
        and install up to two network adapters in a workstation. This ODI
        driver supports the Port, Node Address, Protocol and Frame options
        for creating your own NET.CFG file. For more information on these
        keywords, please refer to Novell's "NetWare ODI shell for DOS -
        NET.CFG options". This installation assumes that the PCMCIA drivers
        are working properly.

 Requirements
 ------------
        .A PCMCIA compatible Laptop
        .A PCMCIA chipset that is PCIC compatible (Intel, Cirrus, Vadem, and
         VLSI) or a Card Service has been installed
        .Netware Lite network operating system
        .A PCMCIA Fast Ethernet Card
        .A knowledge of basic DOS commands and editing text files

 Minimum Skill Level
 -------------------
        .A knowledge of basic DOS commands
        .A knowledge of editing text files
        .A knowledge of DOS basic file structure (CONFIG.SYS and AUTOEXEC.BAT)
        .A knowledge of the network driver configuration being used
        .Please see Support Options if you are not comfortable will this
         skill level

 Getting Started
 ---------------
        1. Follow the normal installation procedure as described by NetWare
           Lite. When prompted for a network driver, simply choose "NOVELL
           NE2000".

        2. After completion of the installation procedure, modify the following
           lines in your STARTNET.BAT file from:

                  LSL
                  NE2000
                  IPXODI A
                  CLIENT
        to:
                  LSL
                  LE100ODI
                  IPXODI A
                  CLIENT

        3. Append the <PATH>\NET.CFG file to the NWLITE directory.  This
           directory was created when you installed NetWare Lite.  <PATH>
           is the directory where NET.CFG resides.

        4. Run STARTNET to access the Novell network.

